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ultimate pressure
Model pumping rate Intake caliber Exhaust caliber with power Cooling water quantity Weight
Pa Tarr

H-150GK 6 4.5 x 1072 100 100 100 11 200 825




