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ultimate pressure
Model pumping rate Intake caliber Exhaust caliber with power Cooling water quantity Weight
Pa Tarr

H-70G(B) 65 5x 102 70 80 50 55 150 525




