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ultimate pressure
Model pumping rate Intake caliber Exhaust caliber with power Cooling water quantity Weight
Pa Tarr

H-80GK 6 45x102 80 80 80 75 150 580




