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The titanium alloy screw vacuum pump is a special application product for harsh corrosive conditions. The flow surfaces inside the pump are all made of high-quality and high-performance titanium alloy materials, featuring excellent corrosion resistance, high strength, and good stability. The combination of titanium and oxygen is extremely strong, and the surface of the titanium alloy easily forms a dense oxide film, providing the part surface with strong anti-corrosion capabilities. Practical cases have shown that the titanium alloy pump is suitable for extracting most corrosive media such as hydrogen chloride, thionyl chloride, nitric acid, organic acids, bases, and inorganic salts.
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Ultimate Pressure Pumping Speed Motor Power

Vodel (50/60Hz) (50/60Hz) Inlet Diam.  Outlet Diam. e Cooling Water Consumpion Weight
(mm) (mm) (50/60Hz) (L/min) (kg)
Torr Pa m3/Hr s
L6701 250/300 70/84 80 40 7515 25 350
LG150T o 540/645  150/180 150 65 185185 3 520
- 525
LGB110T B 400/480 1101132 80 4 75/15 26 350
LGB220T 792/950  220/264 150 65 185/22 3 520
LGB280T 1008/1210  280/336 150 65 2122 32 520

0.75/0.52 100/70
LGB300T 1080/1290 300/360 150 65 22/22 28 520




