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Characteristics

Due to market demand, the screw vacuum pump is equipped with a movable frame and a box-shaped housing. The equipment has the following advantages: The pump is equipped with a movable frame, which enables single-person operation for equipment transfer and fixation, and is suitable for multi-point operation.

The pump is enclosed in a box-shaped housing, which has strong environmental adaptability and a neat and beautiful appearance.

The power supply, cooling water path, gas source gas path, etc. are concentrated on the side panel, making it convenient for customers to disassemble and install.

The pump can be optionally equipped with frequency control, water-cooled motor, temperature monitoring, flow monitoring, etc., with high stability.

The pump can be optionally equipped with PLC control, wireless Wifi and Modbus standard communication protocols, facilitating mobile data exchange.
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Model

XSLGS0

XSLG70

XSLG110

XSLG150

XSLG150A

XSLG200

XSLG300

XSLG300A

XSLGB70

XSLGB110

XSLGB160
XSLGB220

XSLGB220A

XSLGB330

XSLGB450

XSLGB280

XSLGB300

XSLGB400

RS
Ultimate Pressure
(50/60Hz)

Torr Pa
0015 2
/ 7

0.0075 1
0.75/0.52 100/70

0015 2

/ /

0.0075 1
0.75/0.52 100/70

i
Ultimate Pressure
(50/60Hz)
m/Hr s
180/216 50/60
2507300 70/84
400/480 110/132
540/650 150/180
540/650 150/180
720/850 200/240
1080/1290 300/360
1080/1290 300/360
2507300 70/84
400/480 110/132
576/690 160/192
792/950 220/264
792/950 220/264
1188/1425 330/396
1620/1944 450/540
1008/1210 280/336
1008/1290 300/360
1440/1728 4007480

priaginiag
Inlet

Diameter
(mm)

65

80

100

150

150

150

200

150

65

80

100
150

150

65

80

100

150

150

HeOE
Outlet
Caliber

(mm)

40
40
65
65

80780
65
80
65
40
40

65
65

8080
65
80
65
65

65

EeANE
wotor
Power

(kw)
(50/60Hz)
75/15
75/15
1715
18.5/18.5
18.5/18.5
22/22
3037
30/37
75/15
75/15

15/15
18.5/22

18.5/22
30130
45/45
22/22
22/22

371137

SR
Cooling Water
Consumption

(L/min)

25
26

28

55
28
25
25

28

e
Weight
(kg)

295
350
480
520
800
680
950
680
295
350

480
520

800
680
950
520
520

680




