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Unit Model
Model

JZJLGB1200-
8T

Pump model

Pump Model
Main Front
pump pump
Brief Backing
Pump Pump

ZJ1200S LGB110

Pumping
Pumping
Speed
(L9)

1200

ultimate pressure
Ultimate Pressure
(Pa)

0.2

Intake
Caliber Inlet
Diam.
(mm)

250

Exhaust
Outlet
Diam.
(mm)

40

Cooling water
quantity
Cooling Water
Consumption
(L/min)

1250

Motor power
Motor Power(kW)

Main Front
pump pump
Brief Backing
Pump Pump
11 1785




